
# Description

PS 2410 is a “battery backed” auxiliary power supply unit for use in 24 VDC fire systems. It is intended for internal use in domestic and commercial premises. NOTE: The unit MUST be GROUNDED!

**PS 2410**

Power Supply Unit

# Technical and Environmental Specifications

Input voltage . . 220-240 VAC, 50-60 Hz

Nominal output 27.2 VDC

Output voltage 27.2 VDC adjustable

Output current 1A max @ 27.2 VDC

Internal fault output Low voltage +F 27mA nominal

External indication Green - Mains ON

Mains fuse 0,62 A 20mm

Battery fuse 1 A 20mm

Battery provision x 7 Ah max

Tamper Box mounted tamper

Construction Power Coated Steel

Dimensions 300x210x80mm

# Compatible Product Range

* **SensoMAG Series** - Conventional devices
* **SensoIRIS Series -** Addressable devices

# Packing Information

* **Single packing box** - 1 unit PS 2410 Power Supply Unit, dimensions 345x225x90mm
* **Carton packing box** - 5 units PS 2410 Power Supply Unit, dimensions 520x250x367mm

24V

Battery 12V

**Connecting cable**

Battery 12V

Contact Information:

**Teletek Electronics JSC**

14A Srebarna Str, 1407 Sofia, Bulgaria

Tel.:+359 2 9694 800

Fax: +359 2 9625 213

info@teletek-electronics.bg [www.teletek-electronics.com](http://www.teletek-electronics.com/)